
**Setup Grandstream GXP2100 for FPL- Part one- basics**

The IP will be displayed on the main screen, open the browser and type <http://ipdaddress>


The password is admin




Next, you will see the status page




Click on Account1->General settings




Setup your VoIP unlock credentials and click on Save and apply




Next, click on Network settings




Select “Keep alive” and click on Save and apply



Next, click on SIP settings-






Save and apply!

Next, click on Security




Save and apply changes

Next, go to Account1->Audio settings



Apply all changes!

Finally, click on Account1->Status



Setup is now complete and you can start making/receiving calls!